Router: RouterA

Test command: show ip route

The expect ouput is:

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B – BGP

The actual output is:

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B – BGP

Success

-------------------------------------------------------------

Router: RouterB

Test command: ping 172.17.0.1

The expect ouput is:

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B – BGP

The actual output is:

Codes: C - connected, S - static, I - IGRP, R - RIP, M - mobile, B – BGP

Fail

-------------------------------------------------------------

Success: 1 Fail: 1